Impulse must not exceed 10 m/s/s.

Spring constant must be 40.

Damping coefficient must be 10 or less.